# Adding EIPs to a Shared Bandwidth

#### Scenarios

Add EIPs to a shared bandwidth and the EIPs can then share that bandwidth. You can add multiple EIPs to a shared bandwidth at the same time.

#### Notes and Constraints

- After an EIP is added to a shared bandwidth, the original bandwidth used by the EIP will become invalid and the EIP will start to use the shared bandwidth.
- The EIP's original dedicated bandwidth will be deleted.
- Do not add EIPs of the dedicated load balancer type and other types to the same shared bandwidth. Otherwise, the bandwidth limit policy will not take effect.

#### Procedure

1. Log in to the management console.

2. Click in the upper left corner and select the desired region and project.
3. On the console homepage, under Network, click Elastic IP.
4. In the navigation pane on the left, choose Elastic IP and Bandwidth > Shared Bandwidths.
5. In the shared bandwidth list, locate the row that contains the shared bandwidth to which you want to add EIPs. In the Operation column, choose More > Add EIP, and select the EIPs to be added.
   Figure 1 Add EIP
6. Click OK.

Parent topic: Shared Bandwidth