# Querying Bandwidths

#### Function

This API is used to query bandwidths using search criteria.

#### URI

GET /v1/{project_id}/bandwidths

Table 1 describes the parameters.

Table 1 Parameter description
Name | Mandatory | Type | Description
--- | --- | --- | ---
project_id | Yes | String | Specifies the project ID.

marker

No

String

Specifies a resource ID for pagination query, indicating that the query starts from the next record of the specified resource ID.

This parameter can work together with the parameter limit.

- If parameters marker and limit are not passed, all resource records will be returned.
- If the parameter marker is not passed and the value of parameter limit is set to 10, the first 10 resource records will be returned.
- If the value of the parameter marker is set to the resource ID of the 10th record and the value of parameter limit is set to 10, the 11th to 20th resource records will be returned.
- If the value of the parameter marker is set to the resource ID of the 10th record and the parameter limit is not passed, resource records starting from the 11th records (including 11th) will be returned.

limit | No | Integer | Specifies the number of records that will be returned on each page. The value is from 0 to intmax. limit can be used together with marker. For details, see the parameter description of marker.

enterprise_project_id

No

String

- Specifies the enterprise project ID. This field can be used to filter out the VPCs associated with a specified enterprise project.
- The value is 0 or a string that contains a maximum of 36 characters in UUID format with hyphens (-). Value 0 indicates the default enterprise project. To obtain the VPCs bound to all enterprise projects of the user, set all_granted_eps.

NOTE:

This parameter is unsupported. Do not use it.

#### Request Message

- Request parameter

  None

- Example request

      GET https://{Endpoint}/v1/{project_id}/bandwidths?limit={limit}&marker={marker}

#### Response Message

- Response parameter

  Table 2 Response parameter
  Name | Type | Description
  --- | --- | ---
  bandwidths | Array of bandwidths objects | Specifies the bandwidth objects. For details, see Table 3.

  Table 3 Description of the bandwidths field
  Name | Type | Description
  --- | --- | ---

  name

  String

  - Specifies the bandwidth name.
  - The value can contain 1 to 64 characters, including letters, digits, underscores (_), hyphens (-), and periods (.).

  size

  Integer

  - Specifies the bandwidth size in Mbit/s.
  - The value ranges from 1 Mbit/s to 1000 Mbit/s by default. (The specific range may vary depending on the configuration in each region. You can see the bandwidth range of each region on the management console.)

  id | String | Specifies the bandwidth ID, which uniquely identifies the bandwidth.

  share_type

  String

  - Possible values are as follows:
    - PER: Dedicated bandwidth
    - WHOLE: Shared bandwidth

  If this parameter is not set, the list of all bandwidths will be returned by default.

  publicip_info

  Array of publicip_info objects

  - Specifies the information about the EIP that uses the bandwidth. For details, see Table 4.

  tenant_id | String | Specifies the project ID.

  bandwidth_type

  String

  - Specifies the bandwidth type.
  - The value can be:
    - share: Shared bandwidth
    - gray: Dedicated load balancer
    - bgp: Dynamic BGP

  charge_mode | String | If the value is traffic, the bandwidth is billed by traffic.
  billing_info | String | Specifies the bill information. If billing_info is specified, the bandwidth is in yearly/monthly billing mode.

  enterprise_project_id

  String

  - Specifies the enterprise project ID. The value is 0 or a string that contains a maximum of 36 characters in UUID format with hyphens (-). Value 0 indicates the default enterprise project. To obtain the bandwidth bound to all enterprise projects of the user, set all_granted_eps.
  - When creating a bandwidth, associate the enterprise project ID with the bandwidth.
  NOTE:

  This parameter is unsupported. Do not use it.

  status

  String

  - Specifies the bandwidth status.
  - Possible values are as follows:
    - FREEZED (Frozen)
    - NORMAL (Normal)

  created_at

  String

  - Specifies the time (UTC) when the bandwidth is created.
  - Format: yyyy-MM-ddTHH:mm:ss

  updated_at

  String

  - Specifies the time (UTC) when the bandwidth is updated.
  - Format: yyyy-MM-ddTHH:mm:ss

  Table 4 publicip_info object
  Name | Type | Description
  --- | --- | ---
  publicip_id | String | Specifies the ID of the EIP that uses the bandwidth.
  publicip_address | String | Specifies the obtained EIP if only IPv4 EIPs are available.

  publicip_type

  String

  - Specifies the EIP type.
  - The value can be 5_bgp (Dynamic BGP), 5_mailbgp (Mail BGP), or 5_gray (Dedicated load balancer, shared load balancer).
  - Constraints:
    - The configured value must be supported by the system.
    - publicip_id is an IPv4 port. If publicip_type is not specified, the default value is 5_bgp.

- Example response

      {
        "bandwidths": [
          {
            "id": "09b99c91-da7c-449f-94e2-f4934c5b2a71",
            "name": "vpngw-f632a7b0-ef50-4ac5-97e9-ddc56b3d5977",
            "size": 200,
            "share_type": "PER",
            "publicip_info": [
              {
                "publicip_id": "2a65923c-7133-415d-ae3b-cf9635a942c5",
                "publicip_address": "10.xx.xx.3",
                "ip_version": 4,
                "publicip_type": "5_bgp",
              }
            ],
            "tenant_id": "26ae5181a416420998eb2093aaed84d9",
            "bandwidth_type": "bgp",
            "charge_mode": "traffic",
            "billing_info": "",
            "enterprise_project_id": "0",
            "status": "NORMAL"
          },
          {
            "id": "0a583ff1-b43e-4000-ade3-e7af0097f832",
            "name": "vpngw-7e880d5b-f458-40ad-a7e5-735c44cd8b7d",
            "size": 300,
            "share_type": "PER",
            "publicip_info": [
              {
                "publicip_id": "c754bc9a-16d5-4763-9674-d7561917aa80",
                "publicip_address": "10.xx.xx.9",
                "ip_version": 4,
                "publicip_type": "5_bgp",
              }
            ],
            "tenant_id": "26ae5181a416420998eb2093aaed84d9",
            "bandwidth_type": "bgp",
            "charge_mode": "traffic",
            "billing_info": "",
            "enterprise_project_id": "0",
            "status": "NORMAL"
          },
          {
            "id": "0a673f00-3640-4a13-949e-7049b2916baf",
            "name": "bandwidth123",
            "size": 10,
            "share_type": "PER",
            "publicip_info": [
              {
                "publicip_id": "cec7fb70-2f82-4561-bd83-2121fb642fdc",
                "publicip_address": "10.xx.xx.184",
                "ip_version": 4,
                "publicip_type": "5_bgp",
              }
            ],
            "tenant_id": "26ae5181a416420998eb2093aaed84d9",
            "bandwidth_type": "bgp",
            "charge_mode": "traffic",
            "billing_info": "",
            "enterprise_project_id": "0",
            "status": "NORMAL"
          },
          {
            "id": "0dde1eae-1783-46dc-998c-930fbe261ff9",
            "name": "bandwidth123",
            "size": 100,
            "share_type": "PER",
            "publicip_info": [
              {
                "publicip_id": "24232038-e178-40ad-80e4-5abb75db84be",
                "publicip_address": "10.xx.xx.101",
                "ip_version": 4,
                "publicip_type": "5_bgp",
              }
            ],
            "tenant_id": "26ae5181a416420998eb2093aaed84d9",
            "bandwidth_type": "bgp",
            "charge_mode": "traffic",
            "billing_info": "",
            "enterprise_project_id": "0",
            "status": "NORMAL"
          }
        ]
      }

#### Status Code

See Status Codes.

#### Error Code

See Error Codes.

Parent topic: Bandwidth