# Viewing a VPC Flow Log

#### Scenarios

View information about your flow log record.

The capture window is approximately 10 minutes, which indicates that a flow log record will be generated every 10 minutes. After creating a VPC flow log, you need to wait about 10 minutes before you can view the flow log record.

If an ECS is in the stopped state, its flow log records will not be displayed.

#### Procedure

1. Log in to the management console.

2. Click in the upper left corner and select the desired region and project.

3. On the console homepage, under Network, click Virtual Private Cloud.
4. In the navigation pane on the left, choose VPC Flow Logs.
5. Locate the target VPC flow log and click View Log Record in the Operation column to view information about the flow log record in LTS.
   Figure 1 Viewing a log record
   Figure 2 Flow log record

   The flow log record is in the following format:

       <version> <project-id> <interface-id> <srcaddr> <dstaddr> <srcport> <dstport> <protocol> <packets> <bytes> <start> <end> <action> <log-status>

   Example 1: The following is an example of a flow log record in which data was recorded during the capture window:

       1 5f67944957444bd6bb4fe3b367de8f3d 1d515d18-1b36-47dc-a983-bd6512aed4bd 192.168.0.154 192.168.3.25 38929 53 17 1 96 1548752136 1548752736 ACCEPT OK

   Value 1 indicates the VPC flow log version. Traffic with a size of 96 bytes to NIC 1d515d18-1b36-47dc-a983-bd6512aed4bd during the past 10 minutes (from 16:55:36 to 17:05:36 on January 29, 2019) was allowed. A data packet was transmitted over the UDP protocol from source IP address 192.168.0.154 and port 38929 to destination IP address 192.168.3.25 and port 53.

   Example 2: The following is an example of a flow log record in which no data was recorded during the capture window:

       1 5f67944957444bd6bb4fe3b367de8f3d 1d515d18-1b36-47dc-a983-bd6512aed4bd - - - - - - - 1431280876 1431280934 - NODATA

   Example 3: The following is an example of a flow log record in which data was skipped during the capture window:

       1 5f67944957444bd6bb4fe3b367de8f3d 1d515d18-1b36-47dc-a983-bd6512aed4bd - - - - - - - 1431280876 1431280934 - SKIPDATA

   Table 1 describes the fields of a flow log record.

   Table 1 Log field description
   Field | Description | Example Value
   --- | --- | ---
   version | The VPC flow log version. | 1
   project-id | The project ID. | 5f67944957444bd6bb4fe3b367de8f3d
   interface-id | The ID of the NIC for which the traffic is recorded. | 1d515d18-1b36-47dc-a983-bd6512aed4bd
   srcaddr | The source IP address. | 192.168.0.154
   dstaddr | The destination IP address. | 192.168.3.25
   srcport | The source port. | 38929
   dstport | The destination port. | 53
   protocol | The Internet Assigned Numbers Authority (IANA) protocol number of the traffic. For details, see Assigned Internet Protocol Numbers. | 17
   packets | The number of packets transferred during the capture window. | 1
   bytes | The number of bytes transferred during the capture window. | 96
   start | The time, in Unix seconds, of the start of the capture window. | 1548752136
   end | The time, in Unix seconds, of the end of the capture window. | 1548752736

   action

   The action associated with the traffic:
   - ACCEPT: The recorded traffic was allowed by the security groups or firewalls.
   - REJECT: The recorded traffic was denied by the firewalls.

   ACCEPT

   log-status

   The logging status of the VPC flow log:
   - OK: Data is logging normally to the chosen destinations.
   - NODATA: There was no traffic of the Filter setting to or from the NIC during the capture window.
   - SKIPDATA: Some flow log records were skipped during the capture window. This may be caused by an internal capacity constraint or an internal error.

   Example:

   When Filter is set to Accepted traffic, if there is accepted traffic, the value of log-status is OK. If there is no accepted traffic, the value of log-status is NODATA regardless of whether there is rejected traffic. If some accepted traffic is abnormally skipped, the value of log-status is SKIPDATA.

   OK

You can enter a keyword on the log topic details page on the LTS console to search for flow log records.

Parent topic: VPC Flow Log